[:SENSe]:DDEMod:CAPSk:RING:PHASe | command/query

Gets or sets the Phase offset for a single Custom APSK ring.

Command Syntax: | [:SENSe]:DDEMod:CAPSk:RING[1:N]:PHASe <value>
<value> | ::= | Real number
Query Syntax: | [:SENSe]:DDEMod:CAPSk:RING[1:N]:PHASe?
Returns | ::= | Real number
Remarks: | <none>
Version: | 16.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.DigitalDemod.Interfaces.CustomApskRing.Phase

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |