[:SENSe]:C2K:CHANnel:MOD | command/query

Gets or sets the modulation format of the despread channel.

Command Syntax: | [:SENSe]:C2K:CHANnel:MOD <value>
<value> | ::= | "Qpsk" | "Psk8" | "Qam16"
Query Syntax: | [:SENSe]:C2K:CHANnel:MOD?
Returns | ::= | "Qpsk" | "Psk8" | "Qam16"
Remarks: | <none>
Example: |
    :C2K:CHAN:MOD "Qpsk"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Cdma2000.Interfaces.MeasurementExtension.ChannelModulation Agilent.SA.Vsa.Cdma2000.ChannelModulation

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |