[:SENSe]:DDEMod:FILTer | command/query

Gets or sets the measurement filter applied during the digital demodulation measurement.

Command Syntax: | [:SENSe]:DDEMod:FILTer <value>
<value> | ::= | "None" | "Rectangular" | "RootRaisedCosine" | "Gaussian" | "UserDefined" | "LowPass" | "IS95BasePhaseCompensating" | "Edge"
Query Syntax: | [:SENSe]:DDEMod:FILTer?
Returns | ::= | "None" | "Rectangular" | "RootRaisedCosine" | "Gaussian" | "UserDefined" | "LowPass" | "IS95BasePhaseCompensating" | "Edge"
Remarks: | <none>
Example: |
    :DDEM:FILT "None"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.DigitalDemod.Interfaces.MeasurementExtension.MeasurementFilter Agilent.SA.Vsa.DigitalDemod.MeasurementFilter

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |