[:SENSe]:W16E:ZONE:MAP:NAME | command/query

Gets or sets the name of current OFDMA Map, or specifies the Map to use from the current set of OFDMA Maps.

Command Syntax: | [:SENSe]:W16E:ZONE:MAP:NAME <value>
<value> | ::= | String
Query Syntax: | [:SENSe]:W16E:ZONE:MAP:NAME?
Returns | ::= | String
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Ieee80216Ofdma.Interfaces.MeasurementExtension.MapName

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |