:MMEMory:LOAD:RECording | command

Recall the current recording in the specified format from a file.

Command Syntax: | :MMEMory:LOAD:RECording <fileName>, <format>
<fileName> | ::= | String
<format> | ::= | String
Remarks: | <format> is a String whose value can be one of the following:
    "CSV"    = CSV (Comma delimited) [*.csv]
    "E3238S" = E3238S Time Snapshot [*.cap]
    "MAT"    = MAT-File [*.mat]
    "MAT7"   = MAT-File (HDF5) [*.mat, *.hdf, *.h5]
    "N5110A" = N5110A Waveform [*.bin]
    "N5106A" = N5106A Waveform [*.bin]
    "SDF"    = SDF (Fast) [*.sdf, *.dat]
    "TEXT"   = Text (Tab delimited) [*.txt]
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Recording.RecallFile(String,String)

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |