:TRACe:X:FORMat:UNIT | command/query

Gets or sets the x unit type (Power, Peak, RMS) when Format is RealVsImaginary.

Command Syntax: | :TRACe[1:N]:X:FORMat:UNIT <value>
<value> | ::= | "Auto" | "Peak" | "Rms" | "Power" | "MilliRms"
Query Syntax: | :TRACe[1:N]:X:FORMat:UNIT?
Returns | ::= | "Auto" | "Peak" | "Rms" | "Power" | "MilliRms"
Remarks: | <none>
Example: |
    :TRAC:X:FORM:UNIT "Auto"
Version: | 17.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Trace.XUnit Agilent.SA.Vsa.TraceYUnitType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |