[:SENSe]:W16E:ADVanced:EQUalizer:TRAining | command/query

Gets or sets a value indicating whether the equalizer uses just the channel estimation sequence or the whole analysis region for training.

Command Syntax: | [:SENSe]:W16E:ADVanced:EQUalizer:TRAining <value>
<value> | ::= | "ChanEst" | "ChanEstData" | "ChanEstPilots"
Query Syntax: | [:SENSe]:W16E:ADVanced:EQUalizer:TRAining?
Returns | ::= | "ChanEst" | "ChanEstData" | "ChanEstPilots"
Remarks: | <none>
Example: |
    :W16E:ADV:EQU:TRA "ChanEst"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Ieee80216Ofdma.Interfaces.MeasurementExtension.EqualizerTraining Agilent.SA.Vsa.Ieee80216Ofdma.EqualizerTrainingType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |