[:SENSe]:WCDMa:ADVanced:ACHannel[:THReshold] | command/query

Gets or sets the threshold for active channel detection when not automatic.

Command Syntax: | [:SENSe]:WCDMa:ADVanced:ACHannel[:THReshold] <value>
<value> | ::= | Real number
Query Syntax: | [:SENSe]:WCDMa:ADVanced:ACHannel[:THReshold]?
Returns | ::= | Real number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wcdma.Interfaces.MeasurementExtension.ActiveChannelThreshold

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |