[:SENSe]:MBOFdm[:FORMat]:PRESet | command

Preset all measurement attributes to default values for indicated TFC.

Command Syntax: | [:SENSe]:MBOFdm[:FORMat]:PRESet <tfc>
<tfc> | ::= | "Tfc1" | "Tfc2" | "Tfc3" | "Tfc4" | "Tfc5" | "Tfc6" | "Tfc7" | "Tfc8" | "Tfc9" | "Tfc10"
Remarks: | <none>
Example: |
    :MBOF:PRES "Tfc1"
Version: | 15.01 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.MBOfdm.Interfaces.MeasurementExtension.Preset Agilent.SA.Vsa.MBOfdm.TfcType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |