[:SENSe]:GSM[:FORMat]:MODulation:MODE | command/query

Gets or sets how time slots that don't match the specified modulation scheme are handled.

Command Syntax: | [:SENSe]:GSM[:FORMat]:MODulation:MODE <value>
<value> | ::= | "Force" | "Discard"
Query Syntax: | [:SENSe]:GSM[:FORMat]:MODulation:MODE?
Returns | ::= | "Force" | "Discard"
Remarks: | <none>
Example: |
    :GSM:MOD:MODE "Force"
Version: | 14.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.GsmEdgeEvolution.Interfaces.MeasurementExtension.ManualModulationSchemeMode Agilent.SA.Vsa.GsmEdgeEvolution.ManualModulationSchemeMode

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |