:INPut:RECording:LENGth:EXTRa | command/query

Gets or sets a value indicating whether extra data will be acquired to be able to settle the measurement filters during playback.

Command Syntax: | :INPut:RECording:LENGth:EXTRa <value>
<value> | ::= | 0 | 1
Query Syntax: | :INPut:RECording:LENGth:EXTRa?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :INP:REC:LENG:EXTR 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Recording.IsRecordLengthExtra

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |