:INITiate:CONTinuous | command/query

Gets or sets a value indicating whether the measurement is continuous.

Command Syntax: | :INITiate:CONTinuous <contSweep>
<contSweep> | ::= | 0 | 1
Query Syntax: | :INITiate:CONTinuous?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :INIT:CONT 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Measurement.IsContinuous

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |