:INPut:TRIGger:LEVel:EXTernal | command/query

Gets or sets the external trigger level in volts.

Command Syntax: | :INPut:TRIGger:LEVel:EXTernal <value>
<value> | ::= | Real number
Query Syntax: | :INPut:TRIGger:LEVel:EXTernal?
Returns | ::= | Real number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.InputTrigger.ExternalLevel

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |