[:SENSe]:LTE:ADVanced:EVM | command/query

Gets or sets what EVM Minimization method is employed.

Command Syntax: | [:SENSe]:LTE:ADVanced:EVM <value>
<value> | ::= | "Off" | "ThreeGpp" | "Tracking"
Query Syntax: | [:SENSe]:LTE:ADVanced:EVM?
Returns | ::= | "Off" | "ThreeGpp" | "Tracking"
Remarks: | <none>
Example: |
    :LTE:ADV:EVM "Off"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.EvmMinimization Agilent.SA.Vsa.Lte.EvmMinimizationType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |