[:SENSe]:W16E:ZONE:DEFinition | command/query

Gets or sets the source for the OFDMA analysis definition.

Command Syntax: | [:SENSe]:W16E:ZONE:DEFinition <value>
<value> | ::= | "Map" | "Manual" | "Auto"
Query Syntax: | [:SENSe]:W16E:ZONE:DEFinition?
Returns | ::= | "Map" | "Manual" | "Auto"
Remarks: | <none>
Example: |
    :W16E:ZONE:DEF "Map"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Ieee80216Ofdma.Interfaces.MeasurementExtension.Definition Agilent.SA.Vsa.Ieee80216Ofdma.DefinitionType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |