:TRACe:MARKer:ACP:RRC:CHANnel | command/query

Gets or sets a value indicating whether the ACP filters for the adjacent channels have an RRC shape (true) or a rectangular shape (false).

Command Syntax: | :TRACe[1:N]:MARKer:ACP:RRC:CHANnel <enable>
<enable> | ::= | 0 | 1
Query Syntax: | :TRACe[1:N]:MARKer:ACP:RRC:CHANnel?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :TRAC:MARK:ACP:RRC:CHAN 0
Version: | 13.01 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.AcpAdjacentChannelCollection.IsRrcShape

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |