[:SENSe]:TEDS:ADVanced:TRCK:PILot | command/query

Gets or sets a value indicating whether pilot tracking is enabled.

Command Syntax: | [:SENSe]:TEDS:ADVanced:TRCK:PILot <value>
<value> | ::= | 0 | 1
Query Syntax: | [:SENSe]:TEDS:ADVanced:TRCK:PILot?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :TEDS:ADV:TRCK:PIL 0
Version: | 16.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Teds.Interfaces.MeasurementExtension.IsPilotTrackingEnabled

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |