[:SENSe]:LTE[:FORMat]:DLINk:PDSCh:CELLratio | command/query

Gets or sets the PDSCH Cell Specific Ratio to be applied.

Command Syntax: | [:SENSe]:LTE[:FORMat]:DLINk:PDSCh:CELLratio <value>
<value> | ::= | "One" | "PB0" | "PB1" | "PB2" | "PB3"
Query Syntax: | [:SENSe]:LTE[:FORMat]:DLINk:PDSCh:CELLratio?
Returns | ::= | "One" | "PB0" | "PB1" | "PB2" | "PB3"
Remarks: | <none>
Example: |
    :LTE:DLIN:PDSC:CELL "One"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.PdschCellSpecificRatio Agilent.SA.Vsa.Lte.PdschCellSpecificRatioType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |