[:SENSe]:TEDS:ACP:OFFSet | command/query

Gets or sets a value indicating the offset for ACP filter (in Hz).

Command Syntax: | [:SENSe]:TEDS:ACP:OFFSet <value>
<value> | ::= | Real number
Query Syntax: | [:SENSe]:TEDS:ACP:OFFSet?
Returns | ::= | Real number
Remarks: | <none>
Version: | 16.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Teds.Interfaces.MeasurementExtension.AcpOffset

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |