[:SENSe]:LTE:PROFile:DLINk:USER:PRECoding | command/query

Gets or sets the Precoding format for the DL user.

Command Syntax: | [:SENSe]:LTE:PROFile:DLINk:USER[1:N]:PRECoding <value>
<value> | ::= | "Off" | "TransmitDiversity" | "JointEqualizer" | "SpatialMultiplexing"
Query Syntax: | [:SENSe]:LTE:PROFile:DLINk:USER[1:N]:PRECoding?
Returns | ::= | "Off" | "TransmitDiversity" | "JointEqualizer" | "SpatialMultiplexing"
Remarks: | <none>
Example: |
    :LTE:PROF:DLIN:USER:PREC "Off"
Version: | 14.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.DownlinkUser.Precoding Agilent.SA.Vsa.Lte.SharedChannelDecoderType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |