:TRACe:MARKer:ACP:RRC | command/query

Gets or sets a value indicating whether the ACP filter for the reference channel has an RRC shape (true) or a rectangular shape (false).

Command Syntax: | :TRACe[1:N]:MARKer:ACP:RRC <enabled>
<enabled> | ::= | 0 | 1
Query Syntax: | :TRACe[1:N]:MARKer:ACP:RRC?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :TRAC:MARK:ACP:RRC 0
Version: | 13.01 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.MarkerCollection.IsAcpRrcShape

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |