:INPut:RECording:PLAY:DELay:SECond | query

Gets the trigger delay (in Sec) of the current recording.

Query Syntax: | :INPut:RECording:PLAY:DELay:SECond?
Returns | ::= | Real number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Recording.PlayDelaySec

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |