[:SENSe]:DDEMod:ADVanced:STAR:QAM:RING:TWO | command/query

Gets or sets the ratio between the second Star-QAM ring radius and the inner ring radius.

Command Syntax: | [:SENSe]:DDEMod:ADVanced:STAR:QAM:RING:TWO <value>
<value> | ::= | Real number
Query Syntax: | [:SENSe]:DDEMod:ADVanced:STAR:QAM:RING:TWO?
Returns | ::= | Real number
Remarks: | <none>
Version: | 14.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.DigitalDemod.Interfaces.MeasurementExtension.StarQamRing2Ratio

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |