:INITiate:RECording:WAIT | query

Wait for the recording to complete.

Query Syntax: | :INITiate:RECording:WAIT? [msTimeout]
<msTimeout> | ::= | Integer number
Returns | ::= | 0 | 1
Remarks: | Returns 1 if recording completes successfully or 0 if the specified timeout expires. An optional argument can be specified with the time to wait in milliseconds. If the optional argument is not specified then the default time to wait is 10 seconds.
Example: |
    :INITiate:RECording:WAIT? 20000  //Wait up to 20 seconds for a recording to complete.
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Measurement.WaitForRecordingDone(Int32)

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |