*OPC | command/query

Indicates operation complete.

Command Syntax: | *OPC
Query Syntax: | *OPC?
Returns | ::= | 0 | 1
Remarks: | The current implementation of *OPC only works for operations that finish when the measurment completes. It currently just waits until the measurement is done.
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Measurement.IsMeasurementDone

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |