[:SENSe]:W16E[:FORMat]:PREamble:INDex | command/query

Gets or sets which preamble sequence to expect for the downlink subframe. Applies only if the subframe type is Downlink.

Command Syntax: | [:SENSe]:W16E[:FORMat]:PREamble:INDex <value>
<value> | ::= | Integer number
Query Syntax: | [:SENSe]:W16E[:FORMat]:PREamble:INDex?
Returns | ::= | Integer number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Ieee80216Ofdma.Interfaces.MeasurementExtension.PreambleIndex

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |