[:SENSe]:W11A:ADVanced:SUBCarrier:SELection | command/query

Gets or sets which subcarriers to analyze.

Command Syntax: | [:SENSe]:W11A:ADVanced:SUBCarrier:SELection <value>
<value> | ::= | "All" | "Single" | "Pilots"
Query Syntax: | [:SENSe]:W11A:ADVanced:SUBCarrier:SELection?
Returns | ::= | "All" | "Single" | "Pilots"
Remarks: | <none>
Example: |
    :W11A:ADV:SUBC:SEL "All"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wlan80211Agjp.Interfaces.MeasurementExtension.SubcarrierSelection Agilent.SA.Vsa.Wlan80211Agjp.SubcarrierSelection

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |