:INPut:DIGital[:FREQuency]:SRATe | command/query

Gets or sets the sample rate of the digital input.

Command Syntax: | :INPut:DIGital[:FREQuency]:SRATe <srateBaseUnits>
<srateBaseUnits> | ::= | Real number
Query Syntax: | :INPut:DIGital[:FREQuency]:SRATe?
Returns | ::= | Real number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Digital.SampleRate

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |