:TRACe:MARKer:TYPE | command/query

Gets or sets how markers can be positioned and offset.

Command Syntax: | :TRACe[1:N]:MARKer[1:N]:TYPE <markerType>
<markerType> | ::= | "Normal" | "Delta" | "Fixed"
Query Syntax: | :TRACe[1:N]:MARKer[1:N]:TYPE?
Returns | ::= | "Normal" | "Delta" | "Fixed"
Remarks: | <none>
Example: |
    :TRAC:MARK:TYPE "Normal"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Marker.Position Agilent.SA.Vsa.MarkerPositionType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |