:TRACe:DEMod:TABLe:BITorder | command/query

Gets or sets the bit ordering for a digital demodulation symbol table.

Command Syntax: | :TRACe[1:N]:DEMod:TABLe:BITorder <value>
<value> | ::= | "Auto" | "MsbFirst" | "LsbFirst"
Query Syntax: | :TRACe[1:N]:DEMod:TABLe:BITorder?
Returns | ::= | "Auto" | "MsbFirst" | "LsbFirst"
Remarks: | <none>
Example: |
    :TRAC:DEM:TABL:BIT "Auto"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Trace.DemodTableBitOrder Agilent.SA.Vsa.TraceTableBitOrder

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |