[:SENSe]:LTE:PROFile:ULINk:USER:ADD | command

Creates a new downlink user or uplink user.

Command Syntax: | [:SENSe]:LTE:PROFile:ULINk:USER:ADD <userName>
<userName> | ::= | String
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.UserCollection`1.Create

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |