[:SENSe]:FREQuency:CENTer | command/query

Gets or sets the measurement center frequency, in Hertz.

Command Syntax: | [:SENSe]:FREQuency:CENTer <value>
<value> | ::= | Real number
Query Syntax: | [:SENSe]:FREQuency:CENTer?
Returns | ::= | Real number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Frequency.Center

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |