:TRACe:GRAPh:COMPensate:PHASe:ERRor:SPERcent | command/query

Gets or sets the phase error compensation filter bandwidth as a % of span.

Command Syntax: | :TRACe[1:N]:GRAPh:COMPensate:PHASe:ERRor:SPERcent <value>
<value> | ::= | Real number
Query Syntax: | :TRACe[1:N]:GRAPh:COMPensate:PHASe:ERRor:SPERcent?
Returns | ::= | Real number
Remarks: | <none>
Version: | 17.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Graph.PhaseErrorCompensateSpanPercent

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |