# Error Codes

The 89600 VSA SCPI interface logs errors to the system error log (SYST:ERR? query). The following table lists the possible error codes for the 89600 VSA SCPI interface, their numerical codes, and the reason for the error.

-113 | UndefinedHeader | Unknown command.
-102 | SyntaxError | SCPI arguments not in the proper format.
100 | UnhandledException | An unhandled exception occurred when accessing the 89600 VSA .NET interface (SCPI commands are translated to .NET API calls).
130 | ConnectionError | Error when trying to connect to the 89600 VSA application.
140 | ObjectNotFound | Could not find a type in the 89600 VSA .NET API. Typically used when a .NET Enum could not be found that matched the enum name specified as a string argument of a SCPI command.
150 | NotValidForCurrentConfig | A command could not be executed due to the current state of the 89600 VSA application.
160 | InvalidArgument | SCPI command arguments are invalid.
161 | InvalidUnits | Units specified for SCPI command argument are invalid.
162 | InvalidIndex | Index specified in SCPI command argument is invalid.
200 | Deprecated | Indicates that something in a command or query has been deprecated.

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |