[:SENSe]:DDEMod:COMPensate:EQUalize:MODE | command/query

Gets or sets the run mode of the Adaptive Equalizer.

Command Syntax: | [:SENSe]:DDEMod:COMPensate:EQUalize:MODE <value>
<value> | ::= | "Run" | "Hold"
Query Syntax: | [:SENSe]:DDEMod:COMPensate:EQUalize:MODE?
Returns | ::= | "Run" | "Hold"
Remarks: | <none>
Example: |
    :DDEM:COMP:EQU:MODE "Run"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.DigitalDemod.Interfaces.MeasurementExtension.EqualizerMode Agilent.SA.Vsa.DigitalDemod.EqualizerMode

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |