:INPut:DIGital[:FREQuency]:CENTer | command/query

Gets or sets the implied center frequency of a digital input.

Command Syntax: | :INPut:DIGital[:FREQuency]:CENTer <freqHz>
<freqHz> | ::= | Real number
Query Syntax: | :INPut:DIGital[:FREQuency]:CENTer?
Returns | ::= | Real number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Digital.Center

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |