:TRACe:MARKer:OBW:POWer | command/query

Gets or sets the fraction of the total power in the signal that is considered "in band".

Command Syntax: | :TRACe[1:N]:MARKer:OBW:POWer <power>
<power> | ::= | Real number
Query Syntax: | :TRACe[1:N]:MARKer:OBW:POWer?
Returns | ::= | Real number
Remarks: | <none>
Version: | 13.01 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.MarkerCollection.ObwPower

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |