:TRACe:DEMod:STATe:SHAPe | command/query

Gets or sets the shape of the digital demodulation ideal state positions.

Command Syntax: | :TRACe[1:N]:DEMod:STATe:SHAPe <value>
<value> | ::= | "None" | "Cross" | "Circle"
Query Syntax: | :TRACe[1:N]:DEMod:STATe:SHAPe?
Returns | ::= | "None" | "Cross" | "Circle"
Remarks: | <none>
Example: |
    :TRAC:DEM:STAT:SHAP "None"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Trace.DemodStateShape Agilent.SA.Vsa.TraceStateShape

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |