[:SENSe]:CUSTomofdm:ADVanced:SYNC[:MODE] | command/query

Gets or sets how the analyzer synchronizes to the measured signal.

Command Syntax: | [:SENSe]:CUSTomofdm:ADVanced:SYNC[:MODE] <value>
<value> | ::= | "TimeCorrelation" | "CyclicPrefix"
Query Syntax: | [:SENSe]:CUSTomofdm:ADVanced:SYNC[:MODE]?
Returns | ::= | "TimeCorrelation" | "CyclicPrefix"
Remarks: | <none>
Example: |
    :CUST:ADV:SYNC "TimeCorrelation"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.CustomOfdm.Interfaces.MeasurementExtension.SynchronizationMode Agilent.SA.Vsa.CustomOfdm.SynchronizationMode

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |