:TRACe:X:CENTer:SPAN | command/query

Gets or sets a value indicating whether all traces show X frequency annotation as center/span rather than start/stop.

Command Syntax: | :TRACe:X:CENTer:SPAN <isXCenterSpan>
<isXCenterSpan> | ::= | 0 | 1
Query Syntax: | :TRACe:X:CENTer:SPAN?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :TRAC:X:CENT:SPAN 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.TraceCollection.IsXCenterSpan

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |