:INITiate:RESTart | command

Causes the measurement to restart. The Average count is reset to 0 and the measurement transitions to the Running State.

Command Syntax: | :INITiate:RESTart
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Measurement.Restart

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |