[:SENSe]:RFID:SYNCsearch:BIT[:PATTern] | command/query

Gets or sets the bit pattern used by sync search when the synchronization search type is user-specified.

Command Syntax: | [:SENSe]:RFID:SYNCsearch:BIT[:PATTern] <value>
<value> | ::= | String
Query Syntax: | [:SENSe]:RFID:SYNCsearch:BIT[:PATTern]?
Returns | ::= | String
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Rfid.Interfaces.MeasurementExtension.SynchronizationSearchBitPattern

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |