[:SENSe]:W16E[:FORMat]:STANdard | command/query

Gets or sets the demod 802.16 OFDMA standard to apply.

Command Syntax: | [:SENSe]:W16E[:FORMat]:STANdard <value>
<value> | ::= | "P80216Cor1Draft2" | "Ieee80216Ofdma"
Query Syntax: | [:SENSe]:W16E[:FORMat]:STANdard?
Returns | ::= | "P80216Cor1Draft2" | "Ieee80216Ofdma"
Remarks: | <none>
Example: |
    :W16E:STAN "P80216Cor1Draft2"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Ieee80216Ofdma.Interfaces.MeasurementExtension.Standard Agilent.SA.Vsa.Ieee80216Ofdma.StandardsType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |