[:SENSe]:LTE:PROFile:ULINk:USER:PUSCh:FORMat | command/query

Gets or sets the PUCCH format for the allocation/channel.

Command Syntax: | [:SENSe]:LTE:PROFile:ULINk:USER[1:N]:PUSCh:FORMat <value>
<value> | ::= | "Format1" | "Format1A" | "Format1B" | "Format2" | "Format2A" | "Format2B" | "Format1Short" | "Format1AShort" | "Format1BShort" | "Format3" | "Format3Short"
Query Syntax: | [:SENSe]:LTE:PROFile:ULINk:USER[1:N]:PUSCh:FORMat?
Returns | ::= | "Format1" | "Format1A" | "Format1B" | "Format2" | "Format2A" | "Format2B" | "Format1Short" | "Format1AShort" | "Format1BShort" | "Format3" | "Format3Short"
Remarks: | <none>
Example: |
    :LTE:PROF:ULIN:USER:PUSC:FORM "Format1"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.AllocationBase.Format Agilent.SA.Vsa.Lte.PucchFormatType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |