:TRACe:MARKer:POLar:FORMat | command/query

Gets or sets if x-vs-y trace formats show markers as real/imaginary or magnitude/phase.

Command Syntax: | :TRACe[1:N]:MARKer:POLar:FORMat <polarFormat>
<polarFormat> | ::= | "MagnitudePhase" | "RealImaginary"
Query Syntax: | :TRACe[1:N]:MARKer:POLar:FORMat?
Returns | ::= | "MagnitudePhase" | "RealImaginary"
Remarks: | <none>
Example: |
    :TRAC:MARK:POL:FORM "MagnitudePhase"
Version: | 13.01 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.MarkerCollection.PolarFormat Agilent.SA.Vsa.MarkersPolar

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |