:INPut:TRIGger:FMASk:LOWer:OFFSet:AMPLitude | command/query

Gets or sets the lower mask amplitude offset from the current Range of the trigger channel.

Command Syntax: | :INPut:TRIGger:FMASk:LOWer:OFFSet:AMPLitude <value>
<value> | ::= | Real number
Query Syntax: | :INPut:TRIGger:FMASk:LOWer:OFFSet:AMPLitude?
Returns | ::= | Real number
Remarks: | <none>
Version: | 17.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.FrequencyMaskTrigger.LowerAmplitudeOffset

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |