[:SENSe]:RFID[:FORMat]:STANdard | query

Gets the standard with which the current setting is comply

Query Syntax: | [:SENSe]:RFID[:FORMat]:STANdard?
Returns | ::= | "EpcGlobalClass1Generation2" | "Iso180004Mode1" | "Iso180006TypeA" | "Iso180006TypeB" | "Iso18092" | "Iso14443TypeA" | "Iso14443TypeB" | "Iso15693" | "None"
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Rfid.Interfaces.MeasurementExtension.Standard

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |