[:SENSe]:RFID:SYNCsearch:TYPE | command/query

Gets or sets the type of sync pattern used by sync search.

Command Syntax: | [:SENSe]:RFID:SYNCsearch:TYPE <value>
<value> | ::= | "Standard" | "Bit"
Query Syntax: | [:SENSe]:RFID:SYNCsearch:TYPE?
Returns | ::= | "Standard" | "Bit"
Remarks: | <none>
Example: |
    :RFID:SYNC:TYPE "Standard"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Rfid.Interfaces.MeasurementExtension.SynchronizationSearchType Agilent.SA.Vsa.Rfid.SynchronizationSearchType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |