[:SENSe]:W16D:TIME:SLENgth | command/query

Gets or sets how much data is acquired from the input hardware.

Command Syntax: | [:SENSe]:W16D:TIME:SLENgth <value>
<value> | ::= | Real number
Query Syntax: | [:SENSe]:W16D:TIME:SLENgth?
Returns | ::= | Real number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Ieee80216Ofdm.Interfaces.MeasurementExtension.SearchLength

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |