:INPut:DIGital:DATA:SCALe:CHANnel | command/query

Get/Set the data scaling factor for part 1 and 2 of the digital input channel data.

Command Syntax: | :INPut:DIGital:DATA:SCALe[1:N]:CHANnel[1:N] <scale>
<scale> | ::= | Real number
Query Syntax: | :INPut:DIGital:DATA:SCALe[1:N]:CHANnel[1:N]?
Returns | ::= | Real number
Remarks: | <none>
Example: |
    // Set the scaling for parts 1 and 2 of channel 1 to 0.5
    INP:DIG:DATA:SCAL1:CHAN1 0.5
    INP:DIG:DATA:SCAL2:CHAN1 0.5
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.DigitalChannel.DataScalePart1

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |